**A Computerized Glow Curve Analysis Software written in C++**

Jeremy M. Hepker\*, Jack ?. Thiesen\*, Kimberlee J. Kearfott\*

Corresponding author: Kimberlee J. Kearfott, Department of Nuclear Engineering and Radiological Sciences, University of Michigan, 2355 Bonisteel Boulevard, Ann Arbor, Michigan 48109-2104 USA

e-mail: kearfott@umich.edu; Telephone: 1 (734) 763-9117; Fax: 1 (734) 763-4540

**Funding sources:** Am I funded??

**Abstract**

?

**Keywords**: dosimetry, first order kinetics, glow curve, Levenberg Marquardt

**Introduction**

**Methods**

***Model and Fitting Method***

***Data input/output***

***Dosimeters***

***Testing***

**Results**

***Goodness of fit***

***Complexity***

**Conclusions**

**Acknowledgements**

**---- EXAMPLE ----**

The authors are especially grateful to Mr. Ali H. Jawad for sharing computer code which was modified to perform the analysis and helping to refine the experimental protocols. The authors wish to also thank Tobias J. Buth, Alexander S. Dawson, Rebecca A. Lynch, Hien Nguyen, Blake D. Rucinski, and Travis Smith, who performed portions of the tedious hands-on work of repeatedly reading out OSLDs during the time the experimental portion of this work was conducted. This work was funded in part by the Consortium for Verification Technology under Department of Energy National Nuclear Security Administration award number DE-NA0002534.

**References**

Abraham SA, Kearfott KJ, Jawad AH, Boria AJ, Buth TJ, Dawson AS, Eng SC, Frank SJ, Green CA, Jacobs ML, Liu K, Miklos JA, Nguyen H,Rafique M, Rucinski BD, Smith T, Tan YL. Design of interrogation protocols for radiation dose measurements using optically stimulated luminescent dosimeters. Health Phys, accepted September 22, 2016.

Benevides L, Romanyukha A, Hull F, Duffy M, Franks S, Voss S, Moscovitch M. Further studies on the light induced fading associated with the application of OSL to personnel dosimetry. Radiat Meas 46: 1810-1812; 2011. DOI: 10.1016/j.radmeas.2011.05.039

Botter-Jensen L, Agersnap LN, Markey BG, McKeever SWS. Al2O3:C as a sensitive OSL dosemeter for rapid assessment of environmental photon dose rates. Radiat Meas 27: 295-298; 1997. DOI: 10.1016/S1350-4487(96)00124-2

Botter-Jensen L, Banerjee D, Jungner H, Murray AS. Retrospective assessment of environmental dose rates using optically stimulated luminescence from Al2O3:C and quartz. Radiat Prot Dosim 84: 537-542; 1999. DOI: 10.1093/oxfordjournals.rpd.a032793

Edmund JM, Andersen CE, Marckmann CJ, Aznar MC, Akselrod MS, Botter-Jensen L. CW-OSL measurement protocols using optical fibre Al2O3:C dosemeters. Radiat Prot Dosim 119: 368-374; 2006. DOI:10.1093/rpd/nci519

Gronchi CC, Cecatti SGP, Pinto TCNO, Caldas LVE. Optical decay of OSL signal of Al2O3:C detectors exposed to different light sources. Nucl Instrum Methods Phys Res B 266: 2915-2917; 2008. DOI: 10.1016/j.nimb.2008.03.139

Harvey JA, Thomas EM, Kearfott KJ. Quantification of various factors influencing the accuracy and precision of thermoluminescent detector calibrations for new and used chip sets. Health Phys 100(5): S79-S91; 2011. DOI: 10.1097/HP.0b013e3181edb823

Harvey JA, Kearfott KJ, Rafique M. Dose response linearity and practical factors influencing minimum detectable dose for various thermoluminescent detector types. J Radioanal Nucl Chem 303:1711-1718; 2015. DOI: 10.1007/s10967-014-3794-6

Hu B, Y. Wang Y, Zealey W. Performance of Al2O3:C optically stimulated luminescence dosimeters for clinical radiation therapy applications. Australas Phys Eng Sci Med 32: 226-232; 2009. DOI: 10.1007/BF03179243

Jursinic PA. Characterization of optically stimulated luminescent dosimeters, OSLDs, for clinical dosimetric measurements. Med Phys 34: 4594-4604; 2007. DOI: 10.1118/1.2804555

Jursinic PA. Changes in optically stimulated luminescent dosimeter (OSLD) dosimetric characteristics with accumulated dose. Med Phys 37:132-140; 2010. DOI: 10.1118/1.3267489

Kearfott KJ, Grupen-Shemansky ME. Positional radiotherapy beam dosimetry using a laser heated thermoluminescent plate. Med Phys 17(3): 429-435; 1990.

Kearfott KJ, Nabelssi BK, Rucker RH, Klingler GW. Evaluation of two thermoluminescent detection systems for medical imaging environments. Health Phys 59(6): 827-836; 1990.

Kearfott KJ, Chesser JM, Mitchell HE, Coombs MA. Apparent dose equivalents resulting from severe heating of film dosimeters. Health Phys 60(4): 597-601; 1991.

Kearfott KJ, Newton JP, Rafique MK. Sorting a large set of heavily used LiF:Mg,Ti thermoluminescent detectors into repeatable subsets of similar response. Appl Radiat Isot 95: 180-187; 2015. DOI: 10.1016/j.apradiso.2014.10.019

Kearfott KJ, West WG, Rafique MK. The optically stimulated luminescence (OSL) properties LiF:Mg,Ti, Li2B4O7:Cu, CaSO4:Tm and CaF2:Mn thermoluminescent materials. Appl Radiat Isot 99(3): 155-161; 2015. DOI: 10.1016/j.apradiso.2015.03.004

Mrcela I, Bokulic T, Izewska J, Budanec M, Frobe A, Kusic Z. Optically stimulated luminescence in vivo dosimetry for radiotherapy: physical characterization and clinical measurements in 60Co beams. Phys Med Biol 56: 6065-6082; 2011. DOI: 10.1088/0031-9155/56/18/018

Omotayo AA, Cygler JE, Sawakuchi GO. The effect of different bleaching wavelengths on the sensitivity of Al2O3:C optically stimulated luminescence detectors (OSLDs) exposed to 6 MV photon beams. Med Phys 39: 5457-5468; 2012. DOI: 10.1118/1.4742865

Parker LW, Harvey JA, Kearfott KJ. An integrated system for the beta, gamma and neutron calibration and storage of thermoluminescent dosimeters for a research laboratory. Health Phys 100(S1): S43-S49; 2011. DOI: 10.1097/HP.0b013e3181e47b11

Simpkins RW, Kearfott KJ. The minimum number of observations necessary to develop an average thermoluminescent dosimeter element correction factor. Radiat Prot Manage 13(6): 55-61; 1997.

Studenski MT, Haverland NP, Kearfott KJ. Simulation, design, and construction of a 137Cs irradiation facility. Health Phys 92(5): S78-S86; 2007. DOI: 10.1097/01.HP.0000253943.69777.a9

Umisedo NK, Yoshimura EM, Gasparian PBR, Yukihara EG. Comparison between blue and green stimulated luminescence of Al2O3:C. Radiat Meas 45: 151-156; 2010. DOI: 10.1016/j.radmeas.2010.02.001

West WG, Kearfott KJ, " Optically Stimulated Luminescence Dosimetry: An Introduction", in Solid State Nuclear Track Detectors and Their Applications, edited by Hardev Singh Virk, Solid State Phenomena Vol. 238, Trans Tech Publications, ISBN-13: 978-3-03835-527-4, pp. 161-173, 2015.

West WG, Kearfott KJ, Bernal SM. The sunlight OSL response of a commercially available *α*-Al2O3:C personnel dosimetry material. Radiat Prot Dosim 119: 344-349; 2006. DOI: 10.1093/rpd/nci691

Yoshizumi MT, Xavier M, Caldas LVE. Influence of thermal and optical treatments on the OSL response of Al2O3:C pellets using blue light stimulation. IEEE Trans Nucl Sci 60: 979-982; 2013. DOI: 10.1109/TNS.2012.2228502

Yukihara EG, McKeever SWS. Optically Stimulated Luminescence Fundamentals and Applications. John Wiley & Sons Ltd; 2011.

Yukihara EG, Gaza R, McKeever SWS, Soares CG. Optically stimulated luminescence and thermoluminescence efficiencies for high-energy heavy charged particle irradiation in Al2O3:C. Radiat Meas 38: 59-70; 2004a. DOI: 10.1016/S1350-4487(03)00251-8

Yukihara EG, Whitley VH, McKeever SWS, Akselrod AE, Akselrod MS. Effect of high-dose irradiation on the optically stimulated luminescence of Al2O3:C. Radiat Meas 38: 317-330; 2004b. DOI:10.1016/j.radmeas.2004.01.033

**Footnotes**

\*University of Michigan, Department of Nuclear Engineering and Radiological Sciences, Ann Arbor, MI 48109-2104